20-7 URBAN TAP WATER CONDITION BY REGION (2008) |  |
Item | Urban Districts | Liyang City | Jintan City
| General Production Capacity of Water Treatment Plant (10000 m3 /day) | 115.5 | 10.0 | 5.0
| Length of Water Supply Piplines (km) | 5524 | 433 | 708
| Total Water Supply (10000 m3) | 23220 | 2413 | 1879
| Water for Production | 5486 | 748 | 595
| Water for Livelihood | 10261 | 1283 | 907
| Population with Access to Tap Water (10000 persons) | 119.68 | 18.00 | 16.80
| Per Capita Daily Comsumption of Tap Water for Livelihood (liter) | 234.90 | 195.31 | 147.90
| Percentage of Population with Access to Tap Water (%) | 100.0 | 100.0 | 100.0