20-10 CONSTRUCTION OF ORGANIC TOWN BY REGION (2007) |  |  |  |
Item | Whole Municipality | Wujin District | Xinbei District | Liyang City | Jintan City
Population, Area and Planning of Organic Towns |  |  |  |  |  |
Number of Organic Towns (unit) |  | 33 | 12 | 6 | 9 | 6
Organic Town With Overall Planning |  | 24 | 4 | 6 | 8 | 6
Built-up Area of The Town (sq.km) |  | 139.44 | 57.93 | 30.04 | 34.93 | 16.54
Registered Population In Built-up Area of The Town (10000 persons) |  | 47.70 | 25.42 | 7.38 | 10.84 | 4.06
Temporary Population In Built-up Area of The Town (10000 persons) |  | 22.85 | 14.52 | 3.87 | 3.04 | 1.41
Residential Housing of Organic Towns |  |  |  |  |  |
Total Floor Space of Buildings of This Year (10000 sq.m) |  | 2053.02 | 956.98 | 421.22 | 492.59 | 182.23
Above mixed structure |  | 1838.75 | 952.70 | 421.22 | 308.66 | 156.17
Floor Space of Buildings Completed of This Year(10000 sq.m) |  | 68.11 | 41.71 | 12.17 | 8.73 | 5.50
Composite Structure |  | 68.02 | 41.71 | 12.17 | 8.73 | 5.41
Per Capita Living Space of Residential Buildings (sq.m) |  | 43.04 | 37.65 | 57.04 | 45.45 | 44.86
Public Buildings & Productive Buildings of Organic Towns |  |  |  |  |  |
Floor Space of Public Buildings at Year-end (sq.m) |  | 670.28 | 429.76 | 47.12 | 118.30 | 75.10
Above mixed structure |  | 636.48 | 429.76 | 47.12 | 106.97 | 52.63
Floor Space of Public Buildings Completed of This Year (sq.m) |  | 29.58 | 21.31 | 2.80 | 3.39 | 2.08
Above mixed structure |  | 28.67 | 21.31 | 2.80 | 3.28 | 1.28
Floor Space of Productive Buildings of This Year (sq.m) |  | 2246.60 | 1420.53 | 488.00 | 219.80 | 118.27
Above mixed structure |  | 2166.96 | 1420.53 | 482.40 | 186.95 | 77.08
Floor Space of Productive Buildings Completed of This Year (sq.m) |  | 214.63 | 157.32 | 20.59 | 20.57 | 16.15
Above mixed structure |  | 212.30 | 157.32 | 20.59 | 18.82 | 15.57
Tap Water Supply of Organic Town |  |  |  |  |  |
Number of Public Tap Water Supply Facilities (unit) |  | 37 | 9 |  | 17 | 11
Daily Capacity of Public Tap Water Supply (10000 m³) |  | 33.63 | 12.69 |  | 15.85 | 5.09
Number of Self-made Tap Water Supply Facilites (unit) |  | 5 | 2 | 2 | 1 |
Daily Capacity of Self-made Tap Water Supply (10000 m³) |  | 0.40 | 0.10 | 0.20 | 0.10 |
Total Annual Volume of Water Supply (10000 tons) |  | 7901.52 | 4247.50 | 735.73 | 1147.40 | 1770.89
Consumption Volume for Livelihood |  | 2681.69 | 1545.20 | 395.54 | 443.80 | 297.15
Consumption Volume for Production |  | 5201.74 | 2702.16 | 340.19 | 695.60 | 1463.79
Length of Water Supply Pipelines (km) |  | 4556 | 1629 | 1168 | 919 | 840
Population with Access to Tap Water (10000 persons) |  | 70.54 | 39.94 | 11.25 | 13.88 | 5.48
Per Capita Daily Consumption of Tap Water for Residential Use (liter) |  | 104.15 | 106.00 | 96.33 | 87.59 | 148.68
Percentage of Population with Access to Tap Water (%) |  | 100 | 100 | 100 | 100 | 100
Public Utilities of Organic Towns |  |  |  |  |  |
Fuel Gas Subscribers (10000 persons) |  | 60.31 | 33.72 | 11.03 | 11.07 | 4.49
Length of Roads (km) |  | 1912.72 | 978.73 | 315.99 | 414.50 | 203.50
Area of Roads (10000 sq.m) |  | 1221.00 | 687.87 | 201.00 | 229.57 | 102.56
Street Lamps (unit) |  | 26937 | 15281 | 1735 | 6543 | 3378
Bridges (uint) |  | 669 | 284 | 124 | 135 | 126
Length of Flood Control Dikes (km) |  | 429.84 | 217.54 | 80.10 | 93.30 | 38.90
Length of Drainage Piplelines (km) |  | 1182 | 512 | 213 | 300 | 157
Length of Discharge Culverts (km) |  | 961 | 909 | 31 | 19 | 2
Parks, Gardens and Green Areas and Environment Sanitation of Organic Towns |  |  |  |  |  |
Coverage Space of Green Areas (hectare) |  | 2448.54 | 1395.60 | 450.00 | 301.54 | 301.40
Green Areas (hectare) |  | 1350.86 | 663.57 | 471.00 | 144.29 | 72.00
Total Area of Public Green Areas (hectare) |  | 447.43 | 252.26 | 81.50 | 74.17 | 39.50
Per Capita Public Green Area (sq.m) |  | 6.34 | 6.32 | 7.24 | 5.34 | 7.21
Percentage of Greenery Coverage (%) |  | 17.56 | 24.1 | 15.7 | 8.6 | 18.2
Ratio of Green Space (%) |  | 9.7 | 11.5 | 15.7 | 4.1 | 4.4
Annual Volumn of Work of Domestic Garbage Disposal (10000 tons) |  | 39.82 | 20.74 | 6.73 | 9.03 | 3.32
Number of Mechinery of Environmental Sanitation (unit) |  | 500 | 304 | 131 | 41 | 24
Public Lavatories (unit) |  | 659 | 340 | 112 | 167 | 40
Construction Investment in Organic Towns |  |  |  |  |  |
Investment Completed (10000 yuan) |  | 375107 | 238533 | 71264 | 41815 | 23495
Residential Housing |  | 91934 | 67138 | 16172 | 4836 | 3788
Public Buildings |  | 26445 | 18659 | 3678 | 2187 | 1921
Productive Buildings |  | 163612 | 115642 | 23638 | 12648 | 11684
Public Utilities |  | 93116 | 37094 | 27776 | 22144 | 6102
Tap Water Supply |  | 9275 | 4368 | 3055 | 1713 | 139
Roads and Bridges |  | 32586 | 6634 | 14606 | 9480 | 1866
Drainage |  | 15025 | 8582 | 213 | 4320 | 1910
Garden & Forestry |  | 13599 | 5282 | 6294 | 1486 | 537
Environmental Sanitation |  | 8889 | 4803 | 1660 | 1395 | 1031
Fiscal Revenue used for Construction of Public Utilities (10000 Yuan) |  | 59671 | 41291 |  | 8371 | 10009
Fiscal Revenue at Town |  | 52469 | 40586 |  | 5170 | 6714
Note: The statistic data of organic towns exclude four towns, such as Hutang, Niutang, Jincheng and Licheng. The ststistic range shall be built-up area. |