20-7 URBAN TAP WATER CONDITION BY REGION (2007) |  |
Item | Urban Districts | Liyang City | Jintan City
General Production Capacity of Water Treatment Plant (10000 m3 /day) |  | 100.5 | 10.0 | 5.0
Length of Water Supply Piplines (km) |  | 4672 | 425 | 647
Total Water Supply (10000 m3) |  | 23636 | 2245 | 1660
Water for Production |  | 5915 | 742 | 453
Water for Livelihood |  | 9721 | 1207 | 873
Population with Access to Tap Water (10000 persons) |  | 122.39 | 17.50 | 16.00
Per Capita Daily Comsumption of Tap Water for Livelihood (litre) |  | 217.61 | 188.98 | 149.46
Percentage of Population with Access to Tap Water (%) |  | 100.0 | 100.0 | 100.0