20-13 ENVIRONMENTAL PROTECTION BY REGION (2006) |  |  |
Item | Whole Municipality |  |  |
Urban Districts | Liyang City | Jintan City
Wastewater Discharged |  |
Total Volume of Industrial Wastewater Discharged (10000 tons) |  | 27300 | 21440 | 3313 | 2547
Volume of Industrial Wastewater up to the Standards |  | 26779 | 20937 | 3305 | 2537
Volume of Chemical Oxygen Demand in Wastwater Discharged (ton) |  | 36216 | 29517 | 3529 | 3170
Percentage of Industrial Wastewater up to the Standards for Discharge (%) |  | 98.1 | 97.7 | 99.8 | 99.6
Waste Gas |  |  |  |
Total Volume of Industrial Waste Gas Emission (10000 m3) |  | 10752777 | 6791272 | 2028132 | 1933373
Volume of Waste Gas from the Processof Production |  | 1147255 | 743966 | 377300 | 25989
Volume of Waste Gas from Fuel Combustion |  | 9605522 | 6047306 | 1650832 | 1907384
Volume of Sulphur Dioxide Emission (ton) |  | 82930 | 57174 | 12270 | 13486
Volume of Soot Emission (ton) |  | 31465 | 21923 | 3172 | 6370
Volume of Industrial Dust Emission (ton) |  | 59396 | 1389 | 36937 | 21070
Industrail Solid Wastes |  |
Volume of Industrial Solid Wastes Produced (10000 tons) |  | 321.87 | 269.02 | 24.35 | 28.50
Volume of Industrial Solid Wastes Utilized (10000 tons) |  | 316.17 | 263.50 | 24.35 | 28.32
Volume of Industrial Solid Wastes Treated (10000 tons) |  | 5.63 | 5.50 |  | 0.13
Percentage of Industrial Solid Wastes Utilized (%) |  | 98.2 | 98.0 | 100.0 | 99.3
Environmental Construction |  |  |  |
Coverage Rate of Nature Reserves (%) |  | 5.1 | 0.1 | 15.0 | 5.0
Coverage Rate of Soot Control Areas (%) |  | 100.0 | 100.0 | 100.0 | 100.0
Coverage Rate of Areas up to Standards for Noise Control (%) |  | 100.0 | 100.0 | 100.0 | 100.0