20-7 URBAN TAP WATER CONDITION BY REGION (2006) |
Item | Urban Districts | Liyang City | Jintan City
General Production Capacity of Water Treatment Plant (10000 m3 /day) | 100.5 | 10.0 | 5.0
Length of Water Supply Piplines (km) | 3808 | 404 | 544
Total Water Supply (10000 m3) | 20940 | 1893 | 1196
Water for Production | 5653 | 710 | 220
Water for Livelihood | 8990 | 1180 | 797
Population with Access to Tap Water (10000 persons) | 120.16 | 16.70 | 14.50
Per Capita Daily Comsumption of Tap Water for Livelihood (litre) | 204.98 | 193.59 | 150.50
Percentage of Population with Access to Tap Water (%) | 100.0 | 100.0 | 100.0