20-2 主要年份市区城市设施水平
URBAN CIVIL FACILITIES IN MAIN YEARS |
指 标 | 2000 | 2005 | 2010 | 2011
Item
人均日生活用水量(升) | Per Capita Daily Consumption of Tap Water for Rrsidential Use (liter) | 224.2 | 181.6 | 238.7 | 229.9
自来水普及率(%) | Percentage of Population with Access to Tap Water (%) | 100.0 | 92.7 | 100.0 | 100.0
每万人拥有公交车辆(标台) | Average Public Service Vehicles per 10000 Persons (coach) | 15.6 | 9.0 | 13.1 | 14.3
燃气普及率(%) | Percentage of Population with Access to Fuel Gas (%) | 99.8 | 92.0 | 99.0 | 99.1
人均拥有道路面积(平方米) | Per Capita Area of Roads (sq.m) | 10.7 | 17.9 | 22.9 | 23.5
污水处理率(%) | Rate of Sewerage Disposal(%) | 69.0 | 86.8 | 89.8 | 91.7
人均公园绿地面积(平方米) | Per Capita Green Area of Parks (sq.m) | 5.6 | 7.1 | 12.4 | 12.4
建成区绿化覆盖率(%) | Rate of the Green Space in Constructed Areas (%) | 31.7 | 38.8 | 42.2 | 42.2
生活垃圾无害化处理率(%) | Rate of No Harm Disposal of Living Garbage (%) | 50.5 | 92.1 | 100.0 | 100.0