20-7 URBAN TAP WATER CONDITION BY REGION (2009)
Item | Urban Area | Liyang City | Jintan City
General Production Capacity of Water Treatment Plant (10000 m3 /day) | 165.5 | 10.0 | 5.0
Length of Water Supply Piplines (km) | 6201 | 476 | 766
Total Water Supply (10000 m3) | 23633 | 2410 | 1933
Water for Production | 5391 | 809 | 623
Water for Livelihood | 10837 | 1242 | 943
Population with Access to Tap Water (10000 persons) | 127.93 | 18.25 | 17.10
Per Capita Daily Comsumption of Tap Water for Livelihood (litre) | 232.08 | 186.38 | 151.10
Percentage of Population with Access to Tap Water (%) | 100.0 | 100.0 | 100.0